사 양 요 구 서

부서명 : 일반외과

물품분류 번 호	품목번호	품명 (Descriptions)	단위	수량
		초음파기 (Ultrasound system)	set	1

1. 일반적인 요구사양

1. 무상써비스기간이 3년 이상인 제품(트랜듀서포함)

2. 본원의 PACS와 연동이 가능한 제품

3. 모니터의 position 변동이 쉬운 제품

4. 220V, 60Hz의 전원을 사용하는 제품

5. 사용자 편리하도록 설정이 가능한 제품(원터치스위치 혹은 터치 패널)

6. 모니터 크기는 20인치 이상인 제품

7. 원터치로 이미지의 최적화가 가능한 제품

8. CD/DVD로 데이터 백업이 가능한 제품

9. 유방조직추출기와 사용에 최적화 된 제품

2. 사 양

1. Applications

1) Abdominal

2) Small Parts

3) Breast

4) Vascular

2. Imaging Modes

1) 2D grayscale imaging

2) Adaptive  Broadband flow imaging 혹은 Color  Doppler Velocity

3) SonoCT Real-time Compound Imaging 혹은 SieClear spatial Compounding

4) XRES Adaptive Image Processing 혹은 Dynamic  TCE

5) Tissue Harmonic Imaging 가능

6) Tissue Harmonic SonoCT Imaging 혹은 Tissue Harmonic DTCE

7) Color Power Angio Imaging(CPA) 혹은 Color Doppler Eneragy

8) ISCAN with AGC 혹은 TEQ(+Auto doppler optimize)

9) PulsedWaveDoppler 가능

10) High Definition Zoom mode 가능

11) Reconstruction zoom with pan 가능

12) Dupplex and simultaneous 2D/ PW Doppler 가능

13) Independent  Triplex for simultaneous 2D/Color/PW 가능

14) High Q control 혹은 Auto  Doppler

15) Advanced Breast Package 혹은 Custom Tissue Imaging

16) Elastography 혹은 eSie Touch elasticity imaging

17) Elasto-Quantification 혹은 eSie strain ratio

3. Gray Shades 가능

4 Acquisition frame Rate : 500f/s or more

5. User-Centered Design Focus

1) 모니터크기 : 20"  LCD 혹은 21." LED

2) Built-in A/C line conditioner provides isolation from voltage  fluctuations

and electrical noise interference

3) Four high-capacity fans with automatic speed adjustment to  optimize

cooling efficiency with audible noise

6. System Architecture

1) dynamic range : 180dB 혹은 210dB

2) digita lchannels : 57,000channels 혹은 67,392  channels

3) Multi-application workflow Protocols

7. Image Presentation

1) Up / down 가능

2) Left / right 가능

3) Multiple duplex image formats (1/3-2/3, 1/ 2-1/2,  2/3-1/3  ,50/50 and

full screen ) 가능

8. 화질개선 기술

1) Adaptive Broadband flowimaging 혹은 Color  Doppler Velocity

2) Tissue Harmonic Imaging 가능

3) Tissue Harmonic SonoCT Imaging 혹은 Tissue Harmonic DTCE

4) Color Power Angio Imaging(CPA) 혹은 Color Doppler Energy

5) Measurement Tools and General Description

- 2D distance

- 2D circumference/ area by ellipse, continuous trace,  trace by points

- 2D curved-linear distance

- Manual Doppler distance and trace

- Doppler values including PI,RI,S/D indices

6) Cineloop Review 가능

7) ISCAN with AGC 혹은 TEQ  (Doppler포함)

- One - touch image optimization 2D and Doppler 가능

- Operation in conjunction with SonoCT and XRES imaging  Adaptive

Gain Compensation (AGC)

8) IFOCUS Intelligent Focusing technology 혹은 MultiHertz Multiple

Frequency Imaging

9) IOPTIMIZE Intelligent Optimization 혹은 DIMAQ  imaging optimization

10) SonoCT Real-time Compound Imaging 혹은 SieClear  spatial

Compounding

11) XRES Adaptive Image Processing 혹은 Dynamic  TCE

12) Advanced Breast Package

13) Tissue Aberration Correction 혹은  custom  tissue Imaging

14) Elastography 혹은 eSie Touch elasticity imaging

15) Elasto-Quantification 혹은 S2000  eSie Strain Ratio

9. DATA Intelligent Management 혹은 S2000  Integrated Ultrasound

Workstation

10. Connectivity  or DICOM 3.0 Storage /Print / Worklist 가능

3. 구성품

A) 혹은 B)

A)구성품

1. Basic  architecture----------------------------------------- 1ea

- xSTREAM system architecture

- Broadband acoustic beamforming

- 57,000 digital channels

- 180 dB dynamic range

- 1TB hard disk drive

-  integrated CD/DVD

2. Imaging Modes ------------------------------------------각 1ea

- 2D grayscale imaging with advanced pulse   coding, pulse sharping,

- Multivariate Tissue Harmonic Imaging

- Tissue aberration correction

- Coded beamforming with chirp transmit

- Next Generation SonoCT beam-steered   real-time compounding imaing

- Harmonic sonoCT imaging

- Next Generation XRES adaptive image   processing technology

- ISCAN intelligent scanning with one-button TGC, gain and compression

map optimization

- Broadband flow imaging

- Philips Color Power Angio   Imaging(CPA)

- Color compare mode

- Freehand 3D and MPR imaging

- Contrst imaging

3. Adaptive broadband Flow  imaging --------------------------- 1ea

- Automatically adapts transmit and   receive bandwidth processing based

on color box position   providing optimal sensitivity and color resolution

4. Contrast Specific Imaging  (CSI) ------------------------------ 1ea

- System optimized for detecting contrast agent signatures as they are

approved for use

5. Tissue Harmonic Imaging ----------------------------------- 1ea

- Patented pulse inversion phase   candellation technology

- System processing of second harmonic   frequencies in Tissue

6. Color Power Angio Imaging  (CPA) --------------------------- 1ea

- Highly sensitive mode for small vessel   visualization

7. Freehand 3D volume and MPR  imaging ----------------------- 1ea

- Volume display with surface rendering

- Multiplannar view display

8. ISCAN Intelligent  Optimization ------------------------------ 1ea

- One - touch image optimization 2D and   Doppler

9. IFOCUS Intelligent  Focusing technology ----------------------- 1ea

- Automatic computation of beam   characteristics for

selected region of interest

10. IOPTIMIZE Intelligent  Optimization ------------------------- 1ea

- Multiple technologies for one-button approach to automatically and

Instantly adapt system performance for different patient size, flow states       and clinical requirements

11. SonoCT Real-time  Compounding Imaging --------------------- 1ea

- Automatic selection of the number of steering angles based on the user

-select   Res/Speed condition

12. X-RES Imaging ------------------------------------------ 1ea

- MRI Imaging technology

- Enhance tissue continuity

13. Advanced Breast Package ----------------------------------- 1ea

14.Tissue Abberation Correction --------------------------------- 1ea

- Corrects for speed of sound changes

- Sharper spatial resolution

15. Panoramic Imaging ---------------------------------------- 1ea

- Real-time extended field of view composite imaging acquired in SonoCT

image

- Able to acquire composite image in XRES mode

16. Elastography  -------------------------------------------- 1ea

- Strain based elastography for breast   imaging

- Four dynamic range selections for   elastogram display

17. Elasto-Quantification(EQ) ----------------------------------- 1ea

18. Intima Media  Thickness(IMT) Quantification ------------------- 1ea

19. DATA Intelligent  Management ------------------------------ 1ea

- DICOM 3.0 Print and Store capability to   internal drive or DVD/CD

- Selectable compression for jpg and DICOM   loop transfer

20. DICOM Connectivity --------------------------------------- 1ea

- DICOM 3.0 print and store service class   user

- Fully integrated user inteface

- Transceiver included with NetLink

21. L12-5 Broadband Linear  Array Transducer -------------------- 1ea

22. B/W Printer --------------------------------------------- 1ea

23. Operation & Service  Manual -------------------------------- 1ea

24. 초음파검사용 전동침대(2-모터)--------------------------------- 1ea

25. 기타 장비구동에 필요한 악세사리 ------------------------------ 1set

B)구성품

1. Basic System Architecture(ver.3.0)---------------------------- 1 set

2. Basic Imaging Mode -------------------------------------- 1 set

3. QuikStart Standby Mode ------------------------------------ 1set

4. MultiHertz Multiple Frequency Imaging ----------------------- 1 set

5. Native Tissue Harmonic Imaging (THI) ----------------------- 1 set

6. Dicom Connectivity --------------------------------------- 1 set

7. eSieScan Workflow Protocols ------------------------------- 1 set

8. Advanced Sieclear™ Spatial compounding  -------------------- 1 set

9. Dynamic TCE™ tissue contrast enhancement technology ----------1 set

10. TEQ™ ultrasound technology (2D and PW Doppler) ------------- 1 set

11. eSie Touch™ elasticity imaging ----------------------------- 1 set

12. Custom Tissue Imaging ----------------------------------- 1 set

13. AHP(Auto IMT) --------------------------------------- 1 set

14. eSie strain ratio  ---------------------------------------- 1 set

15. 18L6 HD Linear Transducer ------------------------------- 1 set

16. Panorama image ----------------------------------------- 1 set

17. B/W Printer      ------------------------------------------1 ea

18. Operating Manual ---------------------------------------- 1 ea

19. 초음파검사용전동침대(2-motor)------------------------------- 1 ea

20. 기타 장비구동에 필요한 악세사리 ------------------------------ 1set

4. 기타사항

1. 상기 모든 내용을 모두 충족시키는 제품을 납품하여야 하며 납품 후에라도 상기

요구 사항에 맞지 않는 제품을 납품하였을 때에는 장비의 회수 및 결제 대금을 전액

변상하여야 하며 병원에 입은 손해에 대하여 보상하여야 한다.

2. 장비의 검수는 당 의료원의 의공담당자의 참석하에 실시 한 것만을 인정한다.

3. 장비설치 및 납품시 장비의 고장 및 불량이 발생하였을 경우 즉시 신장비로 교체   하여 재 납품 하여야 한다.

4. 무상 및 유상 써비스 기간내에 원외반출 수리시에는 대체장비를 지원하여야 한다.

5. 장비납품 및 설치시 해당병원 장비별로 납품․설치하여야 하며, 정상운영 될 때까

지 초기교육을 실시하며 교육과 관련한 비용 및 장비설치에 따른 제반비용을 부담하여

야 한다.

6. 장비의 사용자의 변경이 생겼을 경우 Operator 교육을 실시하며 그 제반비용은 무상으

로 처리한다.

7. 무상 A/S기간 중 장비운영과 관련한 모든 프로그램의 Up-grade시 장비 제조사로부터

무상 제공하여야 한다.

8. 제품의 포장은 검수시에 개봉한 것만을 인정한다.

9. 납품은 병원이 요구하는 시간과 장소에 납품한다.

10. 장비의 검수는 장비설치 및 셋팅 완료 후에 실시한다.

11. 장비의 무상보증 기간은 장비 설치 및 검수 후부터 시작한다.

12. 사양서에 제시된 기능은 모두 사용이 가능하여야 하며 구성품 중 빠진 부분이 있   더라도 추가 납품한다.

13. 장비 설치시 병원의 설비의 변동이 없이 설치하는 것을 원칙으로 하되 부득이하게

공사 혹은 구조변경이 필요한 경우 병원에 사전에 통보하여야 하며 공사 시공시 병원

의 요청대로 시공하여야 한다. 또한 공사비용은 장비의 납품업체에서 부담한다.